(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions yes)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile no)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue no)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk yes)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "Gerber/drumbadum/")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "/OSC_IN")
	(net 3 "+3.3V")
	(net 4 "/OSC_OUT")
	(net 5 "/NRST")
	(net 6 "Net-(U2-VCAP_1)")
	(net 7 "Net-(U2-VCAP_2)")
	(net 8 "+3.3VA")
	(net 9 "Net-(C25-Pad1)")
	(net 10 "START_BTN")
	(net 11 "MODE_SELECT_BTN")
	(net 12 "Net-(D1-K)")
	(net 13 "Net-(D2-A)")
	(net 14 "Net-(D3-K)")
	(net 15 "Net-(D3-A)")
	(net 16 "unconnected-(J1-D+-Pad3)")
	(net 17 "unconnected-(J1-D--Pad2)")
	(net 18 "unconnected-(J1-ID-Pad4)")
	(net 19 "/SWDIO")
	(net 20 "/SWCLK")
	(net 21 "unconnected-(J3-PadR)")
	(net 22 "unconnected-(J4-PadR)")
	(net 23 "Net-(J5-PadT)")
	(net 24 "Net-(J6-PadR)")
	(net 25 "unconnected-(J6-PadS)")
	(net 26 "CLOCK_IN")
	(net 27 "Net-(Q1-B)")
	(net 28 "/BOOT0")
	(net 29 "MIDI_RECEIVE")
	(net 30 "pot_1")
	(net 31 "pot_2")
	(net 32 "pot_3")
	(net 33 "pot_4")
	(net 34 "pot_5")
	(net 35 "pot_6")
	(net 36 "pot_7")
	(net 37 "pot_8")
	(net 38 "pot_9")
	(net 39 "pot_10")
	(net 40 "pot_11")
	(net 41 "pot_12")
	(net 42 "pot_13")
	(net 43 "pot_14")
	(net 44 "unconnected-(U2-PB9-Pad62)")
	(net 45 "I2S_CLOCK")
	(net 46 "unconnected-(U2-PC7-Pad38)")
	(net 47 "unconnected-(U2-PA8-Pad41)")
	(net 48 "unconnected-(U2-PB4-Pad56)")
	(net 49 "unconnected-(U2-PB14-Pad35)")
	(net 50 "unconnected-(U2-PC9-Pad40)")
	(net 51 "unconnected-(U2-PA11-Pad44)")
	(net 52 "unconnected-(U2-PC8-Pad39)")
	(net 53 "unconnected-(U2-PC6-Pad37)")
	(net 54 "unconnected-(U2-PA12-Pad45)")
	(net 55 "unconnected-(U2-PB15-Pad36)")
	(net 56 "I2S_DATA")
	(net 57 "unconnected-(U2-PD2-Pad54)")
	(net 58 "unconnected-(U2-PA9-Pad42)")
	(net 59 "I2S_WORD_SELECT")
	(net 60 "unconnected-(U2-PB12-Pad33)")
	(net 61 "unconnected-(U2-PC11-Pad52)")
	(net 62 "unconnected-(U2-PC3-Pad11)")
	(net 63 "unconnected-(U2-PC15-Pad4)")
	(net 64 "unconnected-(U2-PB13-Pad34)")
	(net 65 "unconnected-(U2-PC14-Pad3)")
	(net 66 "unconnected-(U4-NC-Pad1)")
	(net 67 "unconnected-(U4-Pad7)")
	(net 68 "unconnected-(U4-NC-Pad4)")
	(net 69 "Net-(C26-Pad1)")
	(net 70 "unconnected-(U2-PC10-Pad51)")
	(net 71 "/DAC/CAPP")
	(net 72 "/DAC/CAPM")
	(net 73 "/DAC/VNEG")
	(net 74 "/DAC/LDOO")
	(net 75 "/DAC/OUT_L")
	(net 76 "/DAC/OUT_R")
	(net 77 "unconnected-(U2-PB10-Pad29)")
	(net 78 "unconnected-(U2-PB11-Pad30)")
	(net 79 "Net-(SW2-A)")
	(net 80 "Net-(SW3-B)")
	(net 81 "unconnected-(SW1-A-Pad1)")
	(net 82 "unconnected-(U2-PC0-Pad8)")
	(net 83 "unconnected-(U2-PB8-Pad61)")
	(net 84 "/MODE_LED")
	(net 85 "unconnected-(U2-PC13-Pad2)")
	(net 86 "/VBUS")
	(net 87 "/VBUS_I")
	(net 88 "unconnected-(J1-Shield-Pad6)")
	(net 89 "unconnected-(J1-Shield-Pad6)_0")
	(net 90 "unconnected-(J1-Shield-Pad6)_1")
	(net 91 "unconnected-(J1-Shield-Pad6)_2")
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 94.945 75.9808)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at -3.124 -0.0348 0)
			(layer "F.SilkS")
		)
		(property "Value" "22u"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C45783"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Drumbadum.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 86 "/VBUS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-323"
		(layer "F.Cu")
		(at 76.03 109.48 180)
		(descr "SOD-323")
		(tags "SOD-323")
		(property "Reference" "D3"
			(at 0 -1.85 180)
			(layer "F.SilkS")
		)
		(property "Value" "1N4148WS"
			(at 0.1 1.9 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_SMD:D_SOD-323"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.vishay.com/docs/85748/1n4148w.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "75V 0.15A Fast Switching Diode, SOD-123"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C2128"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*SOD?123*")
		(sheetname "Interface")
		(sheetfile "Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.85 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.05 0 180)
			(size 0.6 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "Net-(D3-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.05 0 180)
			(size 0.6 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "Net-(D3-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 109.8 105.8 -45)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at -1.887394 0.528916 0)
			(layer "F.SilkS")
		)
		(property "Value" "20p"
			(at 0 1.16 135)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C1554"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Drumbadum.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 135)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 315)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "/OSC_OUT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 315)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 161.436 89.792 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C29"
			(at 1.304 -2.253 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C307331"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Interface")
		(sheetfile "Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "MODE_SELECT_BTN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_USB:USB_Micro_B_MJ_U254051N4BH806"
		(layer "F.Cu")
		(at 86.487 64.084 180)
		(descr "U254-051N-4BH806-2")
		(tags "Connector")
		(property "Reference" "J1"
			(at 6.372 -0.5782 180)
			(layer "F.SilkS")
		)
		(property "Value" "USB_B_Micro"
			(at 0 -6.7 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "Connector_USB:USB_Micro_B_MJ_U254051N4BH806"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "USB Micro Type B connector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C319170"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "USB*")
		(sheetname "Root")
		(sheetfile "Drumbadum.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -1.4 4.9 180)
			(layer "F.Fab")
		)
		(fp_text user "PCB Edge"
			(at -1.75 1.75 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -2 -1.165 180)
			(size 0.001 0.001)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 2 -1.165 180)
			(size 0.001 0.001)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -1.3 -1.985 180)
			(size 0.4 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 87 "/VBUS_I")
			(pinfunction "VBUS")
			(pintype "power_out")
		)
		(pad "2" smd rect
			(at -0.65 -1.985 180)
			(size 0.4 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "unconnected-(J1-D--Pad2)")
			(pinfunction "D-")
			(pintype "bidirectional+no_connect")
		)
		(pad "3" smd rect
			(at 0 -1.985 180)
			(size 0.4 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "unconnected-(J1-D+-Pad3)")
			(pinfunction "D+")
			(pintype "bidirectional+no_connect")
		)
		(pad "4" smd rect
			(at 0.65 -1.985 180)
			(size 0.4 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "unconnected-(J1-ID-Pad4)")
			(pinfunction "ID")
			(pintype "passive+no_connect")
		)
		(pad "5" smd rect
			(at 1.3 -1.985 180)
			(size 0.4 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_out")
		)
		(pad "6" thru_hole oval
			(at -3.575 -2.485 180)
			(size 1.05 1.85)
			(drill oval 0.45 1.25)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 90 "unconnected-(J1-Shield-Pad6)_1")
			(pinfunction "Shield")
			(pintype "passive+no_connect")
		)
		(pad "6" thru_hole oval
			(at -3.575 0.965 180)
			(size 1.05 1.85)
			(drill oval 0.45 1.25)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 89 "unconnected-(J1-Shield-Pad6)_0")
			(pinfunction "Shield")
			(pintype "passive+no_connect")
		)
		(pad "6" thru_hole oval
			(at 3.575 -2.485 180)
			(size 1.05 1.85)
			(drill oval 0.45 1.25)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "unconnected-(J1-Shield-Pad6)_2")
			(pinfunction "Shield")
			(pintype "passive+no_connect")
		)
		(pad "6" thru_hole oval
			(at 3.575 0.965 180)
			(size 1.05 1.85)
			(drill oval 0.45 1.25)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 88 "unconnected-(J1-Shield-Pad6)")
			(pinfunction "Shield")
			(pintype "passive+no_connect")
		)
		(model "U254-051N-4BH806.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "/Users/mortenslingsby/Documents/DIY/5. KiCad lib/USB/XKB Connectivity U254-051N-4BH806.step"
			(offset
				(xyz -3.7 -3.65 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Potentiometer_THT:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical"
		(layer "F.Cu")
		(at 70.8298 87.5 90)
		(descr "Potentiometer, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
		(tags "potentiometer vertical 9mm single")
		(property "Reference" "RV10"
			(at 13.472 2.5762 0)
			(layer "F.SilkS")
		)
		(property "Value" "B10k"
			(at 0 9.86 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Potentiometer_THT:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Potentiometer"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "-"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "Interface")
		(sheetfile "Interface.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.62 2.54 -90)
			(layer "F.Fab")
		)
		(pad "" thru_hole oval
			(at 7.5 -2.3 180)
			(size 2.72 3.24)
			(drill oval 1.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "" thru_hole oval
			(at 7.5 7.3 180)
			(size 2.72 3.24)
			(drill oval 1.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "+3.3VA")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.5 180)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "pot_10")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5 180)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alpha_RD901F-40-00D_Single_Vertical.wrl"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "/Users/mortenslingsby/Documents/DIY/5. KiCad lib/Pot/RD901F-40-15R1-B10K-00DL1/3D/RD901F-40-15R1-B10K-00DL1.stp"
			(offset
				(xyz 7.7 -2.5 -1)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
		(layer "F.Cu")
		(at 94.9075 81.7208 -90)
		(descr "module CMS SOT223 4 pins")
		(tags "CMS SOT")
		(property "Reference" "U1"
			(at 0.52 4.7925 180)
			(layer "F.SilkS")
		)
		(property "Value" "AMS1117-3.3"
			(at 0 4.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.advanced-monolithic.com/pdf/ds1117.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1A Low Dropout regulator, positive, 3.3V fixed output, SOT-223"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C6186"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?223*TabPin2*")
		(sheetname "Root")
		(sheetfile "Drumbadum.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3.15 -2.3 270)
			(size 2 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -3.15 0 270)
			(size 2 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "VO")
			(pintype "power_out")
		)
		(pad "2" smd roundrect
			(at 3.15 0 270)
			(size 2 3.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "VO")
			(pintype "power_out")
		)
		(pad "3" smd roundrect
			(at -3.15 2.3 270)
			(size 2 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 86 "/VBUS")
			(pinfunction "VI")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 109.675 69.6)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R2"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C21190"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Drumbadum.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "Net-(D1-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 59.9038 85.5)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R10"
			(at 3.3422 0.0508 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C25804"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Interface")
		(sheetfile "Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 26 "CLOCK_IN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 111.2 117.475)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R1"
			(at 0.052 1.524 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C25804"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Drumbadum.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 28 "/BOOT0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Potentiometer_THT:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical"
		(layer "F.Cu")
		(at 117 87.5 90)
		(descr "Potentiometer, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
		(tags "potentiometer vertical 9mm single")
		(property "Reference" "RV9"
			(at 13.5228 2.1698 0)
			(layer "F.SilkS")
		)
		(property "Value" "B10k"
			(at 0 9.86 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Potentiometer_THT:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Potentiometer"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "-"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "Interface")
		(sheetfile "Interface.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.62 2.54 -90)
			(layer "F.Fab")
		)
		(pad "" thru_hole oval
			(at 7.5 -2.3 180)
			(size 2.72 3.24)
			(drill oval 1.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "" thru_hole oval
			(at 7.5 7.3 180)
			(size 2.72 3.24)
			(drill oval 1.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "+3.3VA")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.5 180)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "pot_9")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5 180)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alpha_RD901F-40-00D_Single_Vertical.wrl"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "/Users/mortenslingsby/Documents/DIY/5. KiCad lib/Pot/RD901F-40-15R1-B10K-00DL1/3D/RD901F-40-15R1-B10K-00DL1.stp"
			(offset
				(xyz 7.7 -2.5 -1)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "Package_SO:SOP-8_6.605x9.655mm_P2.54mm"
		(layer "F.Cu")
		(at 76.66 118.9 -90)
		(descr "SOP, 8 Pin (https://www.onsemi.com/pdf/datasheet/hcpl2631m-d.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOP SO")
		(property "Reference" "U4"
			(at -0.028 -6.398 180)
			(layer "F.SilkS")
		)
		(property "Value" "6N137S1"
			(at 0 5.78 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:SOP-8_6.605x9.655mm_P2.54mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C110020"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Interface")
		(sheetfile "Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -4.35 -3.81 270)
			(size 2.3 1.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.135135)
			(net 66 "unconnected-(U4-NC-Pad1)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "2" smd roundrect
			(at -4.35 -1.27 270)
			(size 2.3 1.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.135135)
			(net 14 "Net-(D3-K)")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -4.35 1.27 270)
			(size 2.3 1.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.135135)
			(net 15 "Net-(D3-A)")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at -4.35 3.81 270)
			(size 2.3 1.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.135135)
			(net 68 "unconnected-(U4-NC-Pad4)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "5" smd roundrect
			(at 4.35 3.81 270)
			(size 2.3 1.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.135135)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "6" smd roundrect
			(at 4.35 1.27 270)
			(size 2.3 1.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.135135)
			(net 29 "MIDI_RECEIVE")
			(pintype "passive")
		)
		(pad "7" smd roundrect
			(at 4.35 -1.27 270)
			(size 2.3 1.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.135135)
			(net 67 "unconnected-(U4-Pad7)")
			(pintype "passive+no_connect")
		)
		(pad "8" smd roundrect
			(at 4.35 -3.81 270)
			(size 2.3 1.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.135135)
			(net 3 "+3.3V")
			(pinfunction "VCC")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOP-8_6.605x9.655mm_P2.54mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Audio:PJ-320A_PCB"
		(layer "F.Cu")
		(at 45.5214 59.895 -90)
		(property "Reference" "J6"
			(at 8.4455 -3.269 -90)
			(layer "F.SilkS")
		)
		(property "Value" "MIDI_IN"
			(at 8.4455 -4.539 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Audio:PJ-320A_PCB"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Jack"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "-"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Interface")
		(sheetfile "Interface.kicad_sch")
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at 3.7 2.2 270)
			(size 1.1 1.1)
			(drill 1.1)
			(layers "F&B.Cu")
		)
		(pad "" thru_hole oval
			(at 5.15 0 270)
			(size 1.8 1.5)
			(drill oval 1.4 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "" np_thru_hole circle
			(at 10.7 2.2 270)
			(size 1.1 1.1)
			(drill 1.1)
			(layers "F&B.Cu")
		)
		(pad "R" thru_hole oval
			(at 8.25 0 270)
			(size 1.8 1.5)
			(drill oval 1.4 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "Net-(J6-PadR)")
			(pintype "passive")
		)
		(pad "S" thru_hole roundrect
			(at 13.45 4.5 270)
			(size 1.7 1.6)
			(drill oval 1.4 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.1470588235)
			(net 25 "unconnected-(J6-PadS)")
			(pintype "passive+no_connect")
		)
		(pad "T" thru_hole oval
			(at 12.35 0 270)
			(size 1.8 1.5)
			(drill oval 1.4 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(D3-A)")
			(pintype "passive")
		)
		(model "/Users/mortenslingsby/Documents/DIY/5. KiCad lib/PJ-320a/PJ-320A.step"
			(offset
				(xyz 2 -2.4 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "LED_THT:LED_D3.0mm"
		(layer "F.Cu")
		(at 171.963 78.9216 180)
		(descr "LED, diameter 3.0mm, 2 pins")
		(tags "LED diameter 3.0mm 2 pins")
		(property "Reference" "D2"
			(at 1.27 -2.96 180)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 1.27 2.96 180)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_THT:LED_D3.0mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "-"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "Drumbadum.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 180)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(D2-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 111.4 91.75)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C16"
			(at 0.106 1.586 0)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C15849"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Drumbadum.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "+3.3VA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 91.910589 110.789411 -135)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C8"
			(at 2.418462 -1.042983 180)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 -135)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C307331"
			(at 0 0 -135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Drumbadum.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -135)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 225)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 225)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_THTPad_1.5x1.5mm_Drill0.7mm"
		(layer "F.Cu")
		(at 132.68 69.01)
		(descr "THT rectangular pad as test Point, square 1.5mm side length, hole diameter 0.7mm")
		(tags "test point THT pad rectangle square")
		(property "Reference" "TP1"
			(at 0.08 -2.44 0)
			(layer "F.SilkS")
		)
		(property "Value" "Chassis GND"
			(at 0.11 2.51 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "TestPoint:TestPoint_THTPad_1.5x1.5mm_Drill0.7mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Drumbadum.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.65 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.5 1.5)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Potentiometer_THT:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical"
		(layer "F.Cu")
		(at 56.7 129.266266 90)
		(descr "Potentiometer, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
		(tags "potentiometer vertical 9mm single")
		(property "Reference" "RV4"
			(at 13.573 2.482 0)
			(layer "F.SilkS")
		)
		(property "Value" "B10k"
			(at 0 9.86 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Potentiometer_THT:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Potentiometer"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "-"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "Interface")
		(sheetfile "Interface.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.62 2.54 -90)
			(layer "F.Fab")
		)
		(pad "" thru_hole oval
			(at 7.5 -2.3 180)
			(size 2.72 3.24)
			(drill oval 1.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "" thru_hole oval
			(at 7.5 7.3 180)
			(size 2.72 3.24)
			(drill oval 1.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "+3.3VA")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.5 180)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "pot_4")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5 180)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alpha_RD901F-40-00D_Single_Vertical.wrl"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "/Users/mortenslingsby/Documents/DIY/5. KiCad lib/Pot/RD901F-40-15R1-B10K-00DL1/3D/RD901F-40-15R1-B10K-00DL1.stp"
			(offset
				(xyz 7.7 -2.5 -1)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 160 104.525 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R9"
			(at 1.909 -1.732 0)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 0 1.43 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C25803"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Interface")
		(sheetfile "Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "START_BTN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 144.733 121.8692)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R4"
			(at -0.0038 1.7272 0)
			(layer "F.SilkS")
		)
		(property "Value" "470"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C23179"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "DAC")
		(sheetfile "DAC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 75 "/DAC/OUT_L")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "Net-(C25-Pad1)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Potentiometer_THT:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical"
		(layer "F.Cu")
		(at 134 108.383133 90)
		(descr "Potentiometer, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
		(tags "potentiometer vertical 9mm single")
		(property "Reference" "RV6"
			(at 13.885593 2.038807 0)
			(layer "F.SilkS")
		)
		(property "Value" "B10k"
			(at 0 9.86 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Potentiometer_THT:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Potentiometer"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "-"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "Interface")
		(sheetfile "Interface.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.62 2.54 -90)
			(layer "F.Fab")
		)
		(pad "" thru_hole oval
			(at 7.5 -2.3 180)
			(size 2.72 3.24)
			(drill oval 1.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "" thru_hole oval
			(at 7.5 7.3 180)
			(size 2.72 3.24)
			(drill oval 1.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "+3.3VA")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.5 180)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "pot_6")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5 180)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alpha_RD901F-40-00D_Single_Vertical.wrl"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "/Users/mortenslingsby/Documents/DIY/5. KiCad lib/Pot/RD901F-40-15R1-B10K-00DL1/3D/RD901F-40-15R1-B10K-00DL1.stp"
			(offset
				(xyz 7.7 -2.5 -1)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 141.438 119.5026)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R5"
			(at 0 1.6554 0)
			(layer "F.SilkS")
		)
		(property "Value" "470"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C23179"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "DAC")
		(sheetfile "DAC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 76 "/DAC/OUT_R")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 69 "Net-(C26-Pad1)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 60.0308 78.0542 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R7"
			(at -0.0762 -2.0722 180)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C25803"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Interface")
		(sheetfile "Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "Net-(J5-PadT)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 27 "Net-(Q1-B)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 130.773 126.4426)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C20"
			(at 1.053 1.4464 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C307331"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "DAC")
		(sheetfile "DAC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "+3.3VA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Potentiometer_THT:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical"
		(layer "F.Cu")
		(at 143.934993 87.5 90)
		(descr "Potentiometer, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
		(tags "potentiometer vertical 9mm single")
		(property "Reference" "RV7"
			(at 13.631593 2.496007 0)
			(layer "F.SilkS")
		)
		(property "Value" "B10k"
			(at 0 9.86 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Potentiometer_THT:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Potentiometer"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "-"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "Interface")
		(sheetfile "Interface.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.62 2.54 -90)
			(layer "F.Fab")
		)
		(pad "" thru_hole oval
			(at 7.5 -2.3 180)
			(size 2.72 3.24)
			(drill oval 1.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "" thru_hole oval
			(at 7.5 7.3 180)
			(size 2.72 3.24)
			(drill oval 1.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "+3.3VA")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.5 180)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "pot_7")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5 180)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alpha_RD901F-40-00D_Single_Vertical.wrl"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "/Users/mortenslingsby/Documents/DIY/5. KiCad lib/Pot/RD901F-40-15R1-B10K-00DL1/3D/RD901F-40-15R1-B10K-00DL1.stp"
			(offset
				(xyz 7.7 -2.5 -1)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 27.18 151.05)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "REF**"
			(at 0 -4.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "Crystal:Crystal_SMD_HC49-SD"
		(layer "F.Cu")
		(at 116.0018 107.2642 135)
		(descr "SMD Crystal HC-49-SD http://cdn-reichelt.de/documents/datenblatt/B400/xxx-HC49-SMD.pdf, 11.4x4.7mm^2 package")
		(tags "SMD SMT crystal")
		(property "Reference" "Y1"
			(at -0.179605 3.879471 0)
			(layer "F.SilkS")
		)
		(property "Value" "Crystal"
			(at 0 3.55 -45)
			(layer "F.Fab")
		)
		(property "Footprint" "Crystal:Crystal_SMD_HC49-SD"
			(at 0 0 135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Two pin crystal"
			(at 0 0 135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C12674"
			(at 0 0 135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Crystal*")
		(sheetname "Root")
		(sheetfile "Drumbadum.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -45)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -4.25 0 135)
			(size 4.5 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "/OSC_IN")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 4.25 0 135)
			(size 4.5 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "/OSC_OUT")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_HC49-SD.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 96.7232 104.8766 45)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at -1.778091 -1.203354 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 45)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C307331"
			(at 0 0 45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Drumbadum.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 45)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 45)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 48.5 73.725 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R8"
			(at -2.478 -0.268 180)
			(layer "F.SilkS")
		)
		(property "Value" "220"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C22962"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Interface")
		(sheetfile "Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 24 "Net-(J6-PadR)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "Net-(D3-K)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_THT:SW_PUSH_6mm_H8mm"
		(layer "F.Cu")
		(at 167.438 85.7616)
		(descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=8mm")
		(tags "tact sw push 6mm")
		(property "Reference" "SW3"
			(at 3.062 6.9884 0)
			(layer "F.SilkS")
		)
		(property "Value" "Mode select button"
			(at 2.786 6.7 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Button_Switch_THT:SW_PUSH_6mm_H8mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.apem.com/int/index.php?controller=attachment&id_attachment=488"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "MEC 5G single pole normally-open tactile switch"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "-"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SW*MEC*5G*")
		(sheetname "Interface")
		(sheetfile "Interface.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.25 2.25 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 6.5 0 90)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 4.5 90)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 80 "Net-(SW3-B)")
			(pinfunction "B")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 6.5 4.5 90)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 80 "Net-(SW3-B)")
			(pinfunction "B")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H8mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_THT:spdt_mini_MJ"
		(layer "F.Cu")
		(at 93.995 69.6808)
		(property "Reference" "SW1"
			(at 0 -5.25 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SW_SPDT"
			(at 0 5.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Button_Switch_THT:spdt_mini_MJ"
			(at 0 4.5 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 4.5 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Switch, single pole double throw"
			(at 0 4.5 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Drumbadum.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 7 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 -2.54)
			(size 1.8 1.8)
			(drill 1.09)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 81 "unconnected-(SW1-A-Pad1)")
			(pinfunction "A")
			(pintype "passive+no_connect")
		)
		(pad "2" thru_hole circle
			(at 0 0)
			(size 1.8 1.8)
			(drill 1.09)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 87 "/VBUS_I")
			(pinfunction "B")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 2.54)
			(size 1.8 1.8)
			(drill 1.09)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 86 "/VBUS")
			(pinfunction "C")
			(pintype "passive")
		)
		(model "/Users/mortenslingsby/Documents/DIY/5. KiCad lib/spdt-toggle-switch/mini_toggle v1.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 79.9828 125.5 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C28"
			(at 0 -1.627 180)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C307331"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Interface")
		(sheetfile "Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Potentiometer_THT:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical"
		(layer "F.Cu")
		(at 168.188 126.539566 90)
		(descr "Potentiometer, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
		(tags "potentiometer vertical 9mm single")
		(property "Reference" "RV5"
			(at 13.6752 2.627 0)
			(layer "F.SilkS")
		)
		(property "Value" "B10k"
			(at 0 9.86 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Potentiometer_THT:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Potentiometer"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "-"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "Interface")
		(sheetfile "Interface.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.62 2.54 -90)
			(layer "F.Fab")
		)
		(pad "" thru_hole oval
			(at 7.5 -2.3 180)
			(size 2.72 3.24)
			(drill oval 1.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "" thru_hole oval
			(at 7.5 7.3 180)
			(size 2.72 3.24)
			(drill oval 1.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "+3.3VA")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.5 180)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "pot_5")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5 180)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alpha_RD901F-40-00D_Single_Vertical.wrl"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "/Users/mortenslingsby/Documents/DIY/5. KiCad lib/Pot/RD901F-40-15R1-B10K-00DL1/3D/RD901F-40-15R1-B10K-00DL1.stp"
			(offset
				(xyz 7.7 -2.5 -1)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "LED_THT:LED_D3.0mm"
		(layer "F.Cu")
		(at 104.354 69.6158 180)
		(descr "LED, diameter 3.0mm, 2 pins")
		(tags "LED diameter 3.0mm 2 pins")
		(property "Reference" "D1"
			(at 1.27 -2.96 180)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 1.27 2.96 180)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_THT:LED_D3.0mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "-"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "Drumbadum.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 180)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+3.3V")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 108.6 110.5 -45)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 0.494975 -1.555635 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 135)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C307331"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Drumbadum.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 135)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 315)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 315)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Potentiometer_THT:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical"
		(layer "F.Cu")
		(at 29.844 129.266266 90)
		(descr "Potentiometer, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
		(tags "potentiometer vertical 9mm single")
		(property "Reference" "RV13"
			(at 13.5482 2.6016 0)
			(layer "F.SilkS")
		)
		(property "Value" "B10k"
			(at 0 9.86 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Potentiometer_THT:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Potentiometer"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "-"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "Interface")
		(sheetfile "Interface.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.62 2.54 -90)
			(layer "F.Fab")
		)
		(pad "" thru_hole oval
			(at 7.5 -2.3 180)
			(size 2.72 3.24)
			(drill oval 1.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "" thru_hole oval
			(at 7.5 7.3 180)
			(size 2.72 3.24)
			(drill oval 1.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "+3.3VA")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.5 180)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "pot_13")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5 180)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alpha_RD901F-40-00D_Single_Vertical.wrl"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "/Users/mortenslingsby/Documents/DIY/5. KiCad lib/Pot/RD901F-40-15R1-B10K-00DL1/3D/RD901F-40-15R1-B10K-00DL1.stp"
			(offset
				(xyz 7.7 -2.5 -1)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 100.325 81.6008 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C13"
			(at -2.6002 0.005 0)
			(layer "F.SilkS")
		)
		(property "Value" "22u"
			(at 0 1.68 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C45783"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Drumbadum.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 111.45 89.775)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C17"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C15849"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Drumbadum.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 147.623 121.0542 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C25"
			(at -0.1038 2.4402 0)
			(layer "F.SilkS")
		)
		(property "Value" "2.2n"
			(at 0 1.43 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C1604"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "DAC")
		(sheetfile "DAC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "Net-(C25-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Potentiometer_THT:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical"
		(layer "F.Cu")
		(at 43.2962 150.1494 90)
		(descr "Potentiometer, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
		(tags "potentiometer vertical 9mm single")
		(property "Reference" "RV8"
			(at 13.6244 2.1698 0)
			(layer "F.SilkS")
		)
		(property "Value" "B10k"
			(at 0 9.86 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Potentiometer_THT:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Potentiometer"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "-"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "Interface")
		(sheetfile "Interface.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.62 2.54 -90)
			(layer "F.Fab")
		)
		(pad "" thru_hole oval
			(at 7.5 -2.3 180)
			(size 2.72 3.24)
			(drill oval 1.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "" thru_hole oval
			(at 7.5 7.3 180)
			(size 2.72 3.24)
			(drill oval 1.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "+3.3VA")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.5 180)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "pot_8")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5 180)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alpha_RD901F-40-00D_Single_Vertical.wrl"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "/Users/mortenslingsby/Documents/DIY/5. KiCad lib/Pot/RD901F-40-15R1-B10K-00DL1/3D/RD901F-40-15R1-B10K-00DL1.stp"
			(offset
				(xyz 7.7 -2.5 -1)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "Connector_Audio:PJ-320A_PCB"
		(layer "F.Cu")
		(at 172.2 59.9 -90)
		(property "Reference" "J3"
			(at 8.4455 -3.269 -90)
			(layer "F.SilkS")
		)
		(property "Value" "LINE_OUT_L"
			(at 8.4455 -4.539 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Audio:PJ-320A_PCB"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Jack"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "-"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "DAC")
		(sheetfile "DAC.kicad_sch")
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at 3.7 2.2 270)
			(size 1.1 1.1)
			(drill 1.1)
			(layers "F&B.Cu")
		)
		(pad "" thru_hole oval
			(at 5.15 0 270)
			(size 1.8 1.5)
			(drill oval 1.4 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "" np_thru_hole circle
			(at 10.7 2.2 270)
			(size 1.1 1.1)
			(drill 1.1)
			(layers "F&B.Cu")
		)
		(pad "R" thru_hole oval
			(at 8.25 0 270)
			(size 1.8 1.5)
			(drill oval 1.4 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "unconnected-(J3-PadR)")
			(pintype "passive+no_connect")
		)
		(pad "S" thru_hole roundrect
			(at 13.45 4.5 270)
			(size 1.7 1.6)
			(drill oval 1.4 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.1470588235)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "T" thru_hole oval
			(at 12.35 0 270)
			(size 1.8 1.5)
			(drill oval 1.4 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(C25-Pad1)")
			(pintype "passive")
		)
		(model "/Users/mortenslingsby/Documents/DIY/5. KiCad lib/PJ-320a/PJ-320A.step"
			(offset
				(xyz 2 -2.4 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "Potentiometer_THT:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical"
		(layer "F.Cu")
		(at 168.188 145.5418 90)
		(descr "Potentiometer, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
		(tags "potentiometer vertical 9mm single")
		(property "Reference" "RV3"
			(at 13.5198 2.474 0)
			(layer "F.SilkS")
		)
		(property "Value" "B10k"
			(at 0 9.86 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Potentiometer_THT:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Potentiometer"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "-"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "Interface")
		(sheetfile "Interface.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.62 2.54 -90)
			(layer "F.Fab")
		)
		(pad "" thru_hole oval
			(at 7.5 -2.3 180)
			(size 2.72 3.24)
			(drill oval 1.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "" thru_hole oval
			(at 7.5 7.3 180)
			(size 2.72 3.24)
			(drill oval 1.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "+3.3VA")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.5 180)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "pot_3")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5 180)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alpha_RD901F-40-00D_Single_Vertical.wrl"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "/Users/mortenslingsby/Documents/DIY/5. KiCad lib/Pot/RD901F-40-15R1-B10K-00DL1/3D/RD901F-40-15R1-B10K-00DL1.stp"
			(offset
				(xyz 7.7 -2.5 -1)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "Potentiometer_THT:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical"
		(layer "F.Cu")
		(at 78 150.1494 90)
		(descr "Potentiometer, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
		(tags "potentiometer vertical 9mm single")
		(property "Reference" "RV14"
			(at 13.823 2.645 0)
			(layer "F.SilkS")
		)
		(property "Value" "B10k"
			(at 0 9.86 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Potentiometer_THT:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Potentiometer"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "-"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "Interface")
		(sheetfile "Interface.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.62 2.54 -90)
			(layer "F.Fab")
		)
		(pad "" thru_hole oval
			(at 7.5 -2.3 180)
			(size 2.72 3.24)
			(drill oval 1.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "" thru_hole oval
			(at 7.5 7.3 180)
			(size 2.72 3.24)
			(drill oval 1.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "+3.3VA")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.5 180)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "pot_14")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5 180)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alpha_RD901F-40-00D_Single_Vertical.wrl"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "/Users/mortenslingsby/Documents/DIY/5. KiCad lib/Pot/RD901F-40-15R1-B10K-00DL1/3D/RD901F-40-15R1-B10K-00DL1.stp"
			(offset
				(xyz 7.7 -2.5 -1)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 59.1418 82.5777 -90)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q1"
			(at -1.9327 3.0078 180)
			(layer "F.SilkS")
		)
		(property "Value" "MMBT3904"
			(at 0 2.4 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/pzt3904-d.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0.2A Ic, 40V Vce, Small Signal NPN Transistor, SOT-23"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C20526"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "Interface")
		(sheetfile "Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 270)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 27 "Net-(Q1-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 270)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 270)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 26 "CLOCK_IN")
			(pinfunction "C")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Potentiometer_THT:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical"
		(layer "F.Cu")
		(at 141.772 150.1494 90)
		(descr "Potentiometer, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
		(tags "potentiometer vertical 9mm single")
		(property "Reference" "RV2"
			(at 13.4974 2.627 0)
			(layer "F.SilkS")
		)
		(property "Value" "B10k"
			(at 0 9.86 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Potentiometer_THT:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Potentiometer"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "-"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "Interface")
		(sheetfile "Interface.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.62 2.54 -90)
			(layer "F.Fab")
		)
		(pad "" thru_hole oval
			(at 7.5 -2.3 180)
			(size 2.72 3.24)
			(drill oval 1.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "" thru_hole oval
			(at 7.5 7.3 180)
			(size 2.72 3.24)
			(drill oval 1.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "+3.3VA")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.5 180)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "pot_2")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5 180)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alpha_RD901F-40-00D_Single_Vertical.wrl"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "/Users/mortenslingsby/Documents/DIY/5. KiCad lib/Pot/RD901F-40-15R1-B10K-00DL1/3D/RD901F-40-15R1-B10K-00DL1.stp"
			(offset
				(xyz 7.7 -2.5 -1)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 145.123 119.5026)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C26"
			(at -0.47 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "2.2n"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C1604"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "DAC")
		(sheetfile "DAC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 69 "Net-(C26-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 177.41 64.92)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "REF**"
			(at 0 -4.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "F&B.Cu" "*.Mask")
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 108.028996 115.488596 -135)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C12"
			(at -2.311249 -1.169136 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 -135)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C307331"
			(at 0 0 -135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Drumbadum.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -135)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 225)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 225)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
		(layer "F.Cu")
		(at 127.453 122.1726 180)
		(descr "TSSOP, 20 Pin (JEDEC MO-153 Var AC https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U3"
			(at 0 4.4436 180)
			(layer "F.SilkS")
		)
		(property "Value" "PCM5102A"
			(at 0 4.2 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/pcm5102a.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "2.1 VRMS, 112dB Audio Stereo DAC with PLL and 32-bit, 384kHz PCM Interface, TSSOP-20"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C107671"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TSSOP*4.4x6.5mm*P0.65mm*")
		(sheetname "DAC")
		(sheetfile "DAC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.8625 -2.925 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "+3.3VA")
			(pinfunction "CPVDD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -2.8625 -2.275 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 71 "/DAC/CAPP")
			(pinfunction "CAPP")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -2.8625 -1.625 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "CPGND")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -2.8625 -0.975 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 72 "/DAC/CAPM")
			(pinfunction "CAPM")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at -2.8625 -0.325 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 73 "/DAC/VNEG")
			(pinfunction "VNEG")
			(pintype "passive")
		)
		(pad "6" smd roundrect
			(at -2.8625 0.325 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 75 "/DAC/OUT_L")
			(pinfunction "OUTL")
			(pintype "output")
		)
		(pad "7" smd roundrect
			(at -2.8625 0.975 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 76 "/DAC/OUT_R")
			(pinfunction "OUTR")
			(pintype "output")
		)
		(pad "8" smd roundrect
			(at -2.8625 1.625 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "+3.3VA")
			(pinfunction "AVDD")
			(pintype "power_in")
		)
		(pad "9" smd roundrect
			(at -2.8625 2.275 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "AGND")
			(pintype "power_in")
		)
		(pad "10" smd roundrect
			(at -2.8625 2.925 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "DEMP")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at 2.8625 2.925 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "FLT")
			(pintype "input")
		)
		(pad "12" smd roundrect
			(at 2.8625 2.275 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "SCK")
			(pintype "input")
		)
		(pad "13" smd roundrect
			(at 2.8625 1.625 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 45 "I2S_CLOCK")
			(pinfunction "BCK")
			(pintype "input")
		)
		(pad "14" smd roundrect
			(at 2.8625 0.975 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 56 "I2S_DATA")
			(pinfunction "DIN")
			(pintype "input")
		)
		(pad "15" smd roundrect
			(at 2.8625 0.325 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 59 "I2S_WORD_SELECT")
			(pinfunction "LRCK")
			(pintype "input")
		)
		(pad "16" smd roundrect
			(at 2.8625 -0.325 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "FMT")
			(pintype "input")
		)
		(pad "17" smd roundrect
			(at 2.8625 -0.975 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "+3.3VA")
			(pinfunction "XSMT")
			(pintype "input")
		)
		(pad "18" smd roundrect
			(at 2.8625 -1.625 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 74 "/DAC/LDOO")
			(pinfunction "LDOO")
			(pintype "passive")
		)
		(pad "19" smd roundrect
			(at 2.8625 -2.275 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "DGND")
			(pintype "power_in")
		)
		(pad "20" smd roundrect
			(at 2.8625 -2.925 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "DVDD")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 120.47 123.8 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C24"
			(at 0 1.245 180)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C307331"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "DAC")
		(sheetfile "DAC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 74 "/DAC/LDOO")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 132.303 120.02 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C19"
			(at 2.54 -0.01 -90)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C307331"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "DAC")
		(sheetfile "DAC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "+3.3VA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 134.493 125.2326 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C22"
			(at 2.4236 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "2.2u"
			(at 0 1.68 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C377773"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "DAC")
		(sheetfile "DAC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 71 "/DAC/CAPP")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 72 "/DAC/CAPM")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 136.906 125.1826 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C23"
			(at -0.7226 -2.54 180)
			(layer "F.SilkS")
		)
		(property "Value" "2.2u"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C377773"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "DAC")
		(sheetfile "DAC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 73 "/DAC/VNEG")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 102.665 82.1208 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C14"
			(at -0.0482 2.364 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C307331"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Drumbadum.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 134.253 119.1326 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C18"
			(at -0.8824 2.907 0)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.68 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C15850"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "DAC")
		(sheetfile "DAC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "+3.3VA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 85.25 122.5 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R11"
			(at 0 -2.38 180)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C25804"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Interface")
		(sheetfile "Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 29 "MIDI_RECEIVE")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 97.39 122.85 -45)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 0.770394 2.011577 0)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.679999 135)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C15850"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Drumbadum.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 135)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.949999 0 315)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.949999 0 315)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Potentiometer_THT:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical"
		(layer "F.Cu")
		(at 28.3356 87.5 90)
		(descr "Potentiometer, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
		(tags "potentiometer vertical 9mm single")
		(property "Reference" "RV11"
			(at 13.9038 2.5254 0)
			(layer "F.SilkS")
		)
		(property "Value" "B10k"
			(at 0 9.86 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Potentiometer_THT:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Potentiometer"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "-"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "Interface")
		(sheetfile "Interface.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.62 2.54 -90)
			(layer "F.Fab")
		)
		(pad "" thru_hole oval
			(at 7.5 -2.3 180)
			(size 2.72 3.24)
			(drill oval 1.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "" thru_hole oval
			(at 7.5 7.3 180)
			(size 2.72 3.24)
			(drill oval 1.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "+3.3VA")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.5 180)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "pot_11")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5 180)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alpha_RD901F-40-00D_Single_Vertical.wrl"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "/Users/mortenslingsby/Documents/DIY/5. KiCad lib/Pot/RD901F-40-15R1-B10K-00DL1/3D/RD901F-40-15R1-B10K-00DL1.stp"
			(offset
				(xyz 7.7 -2.5 -1)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 104.6226 105.537 -45)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C15"
			(at -1.957696 -0.377171 0)
			(layer "F.SilkS")
		)
		(property "Value" "10n"
			(at 0 1.16 135)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C15195"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Drumbadum.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 135)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 315)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "+3.3VA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 315)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Potentiometer_THT:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical"
		(layer "F.Cu")
		(at 47.3 108.383133 90)
		(descr "Potentiometer, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
		(tags "potentiometer vertical 9mm single")
		(property "Reference" "RV12"
			(at 13.7006 2.3222 0)
			(layer "F.SilkS")
		)
		(property "Value" "B10k"
			(at 0 9.86 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Potentiometer_THT:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Potentiometer"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "-"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "Interface")
		(sheetfile "Interface.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.62 2.54 -90)
			(layer "F.Fab")
		)
		(pad "" thru_hole oval
			(at 7.5 -2.3 180)
			(size 2.72 3.24)
			(drill oval 1.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "" thru_hole oval
			(at 7.5 7.3 180)
			(size 2.72 3.24)
			(drill oval 1.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "+3.3VA")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.5 180)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "pot_12")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5 180)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alpha_RD901F-40-00D_Single_Vertical.wrl"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "/Users/mortenslingsby/Documents/DIY/5. KiCad lib/Pot/RD901F-40-15R1-B10K-00DL1/3D/RD901F-40-15R1-B10K-00DL1.stp"
			(offset
				(xyz 7.7 -2.5 -1)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 93.86 122.22 -135)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C11"
			(at 0.511238 2.551948 0)
			(layer "F.SilkS")
		)
		(property "Value" "2.2u"
			(at 0 1.679999 -135)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 -135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C377773"
			(at 0 0 -135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Drumbadum.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -135)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.949999 0 225)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "Net-(U2-VCAP_2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.949999 0 225)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Potentiometer_THT:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical"
		(layer "F.Cu")
		(at 119.0626 150.1494 90)
		(descr "Potentiometer, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
		(tags "potentiometer vertical 9mm single")
		(property "Reference" "RV1"
			(at 13.599 2.7304 0)
			(layer "F.SilkS")
		)
		(property "Value" "B10k"
			(at 0 9.86 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Potentiometer_THT:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Potentiometer"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "-"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "Interface")
		(sheetfile "Interface.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.62 2.54 -90)
			(layer "F.Fab")
		)
		(pad "" thru_hole oval
			(at 7.5 -2.3 180)
			(size 2.72 3.24)
			(drill oval 1.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "" thru_hole oval
			(at 7.5 7.3 180)
			(size 2.72 3.24)
			(drill oval 1.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "+3.3VA")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.5 180)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "pot_1")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5 180)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alpha_RD901F-40-00D_Single_Vertical.wrl"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "/Users/mortenslingsby/Documents/DIY/5. KiCad lib/Pot/RD901F-40-15R1-B10K-00DL1/3D/RD901F-40-15R1-B10K-00DL1.stp"
			(offset
				(xyz 7.7 -2.5 -1)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 122.86 125.25 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C21"
			(at -1.8744 -0.46 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C307331"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "DAC")
		(sheetfile "DAC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Horizontal"
		(layer "F.Cu")
		(at 106.175 133.925 -90)
		(descr "Through hole angled pin header, 1x05, 2.54mm pitch, 6mm pin length, single row")
		(tags "Through hole angled pin header THT 1x05 2.54mm single row")
		(property "Reference" "J2"
			(at 4.385 -2.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "SWD header"
			(at 4.385 12.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x05, script generated"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "-"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "Drumbadum.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.77 5.08 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/SWCLK")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/NRST")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/SWDIO")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+3.3V")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Audio:PJ-320A_PCB"
		(layer "F.Cu")
		(at 60.1454 59.9 -90)
		(property "Reference" "J5"
			(at 8.4455 -3.269 -90)
			(layer "F.SilkS")
		)
		(property "Value" "CLK_IN"
			(at 8.4455 -4.539 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Audio:PJ-320A_PCB"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Jack"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "-"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Interface")
		(sheetfile "Interface.kicad_sch")
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at 3.7 2.2 270)
			(size 1.1 1.1)
			(drill 1.1)
			(layers "F&B.Cu")
		)
		(pad "" thru_hole oval
			(at 5.15 0 270)
			(size 1.8 1.5)
			(drill oval 1.4 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "" np_thru_hole circle
			(at 10.7 2.2 270)
			(size 1.1 1.1)
			(drill 1.1)
			(layers "F&B.Cu")
		)
		(pad "R" thru_hole oval
			(at 8.25 0 270)
			(size 1.8 1.5)
			(drill oval 1.4 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "S" thru_hole roundrect
			(at 13.45 4.5 270)
			(size 1.7 1.6)
			(drill oval 1.4 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.1470588235)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "T" thru_hole oval
			(at 12.35 0 270)
			(size 1.8 1.5)
			(drill oval 1.4 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "Net-(J5-PadT)")
			(pintype "passive")
		)
		(model "/Users/mortenslingsby/Documents/DIY/5. KiCad lib/PJ-320a/PJ-320A.step"
			(offset
				(xyz 2 -2.4 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "Button_Switch_THT:SW_PUSH_6mm_H8mm"
		(layer "F.Cu")
		(at 173.938 104.3733 180)
		(descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=8mm")
		(tags "tact sw push 6mm")
		(property "Reference" "SW2"
			(at 3.25 -2 180)
			(layer "F.SilkS")
		)
		(property "Value" "Start button"
			(at 3.75 6.7 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Button_Switch_THT:SW_PUSH_6mm_H8mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.apem.com/int/index.php?controller=attachment&id_attachment=488"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "MEC 5G single pole normally-open tactile switch"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "-"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SW*MEC*5G*")
		(sheetname "Interface")
		(sheetfile "Interface.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.25 2.25 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "Net-(SW2-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 6.5 0 270)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "Net-(SW2-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 4.5 270)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "B")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 6.5 4.5 270)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "B")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H8mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 159.785 91.062 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R13"
			(at 0 2.413 180)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C25803"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Interface")
		(sheetfile "Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "MODE_SELECT_BTN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_QFP:LQFP-64_10x10mm_P0.5mm"
		(layer "F.Cu")
		(at 100.368996 112.758596 -135)
		(descr "LQFP, 64 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/ad7606_7606-6_7606-4.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "LQFP QFP")
		(property "Reference" "U2"
			(at 0.129683 -7.97716 0)
			(layer "F.SilkS")
		)
		(property "Value" "STM32F405RGTx"
			(at 0 7.4 -135)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 0 0 -135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f405rg.pdf"
			(at 0 0 -135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 1024KB flash, 192KB RAM, 168 MHz, 1.8-3.6V, 51 GPIO, LQFP64"
			(at 0 0 -135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C15742"
			(at 0 0 -135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LQFP*10x10mm*P0.5mm*")
		(sheetname "Root")
		(sheetfile "Drumbadum.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -135)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -5.675 -3.749999 225)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "VBAT")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -5.675 -3.25 225)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 85 "unconnected-(U2-PC13-Pad2)")
			(pinfunction "PC13")
			(pintype "bidirectional+no_connect")
		)
		(pad "3" smd roundrect
			(at -5.675 -2.75 225)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 65 "unconnected-(U2-PC14-Pad3)")
			(pinfunction "PC14")
			(pintype "bidirectional+no_connect")
		)
		(pad "4" smd roundrect
			(at -5.675 -2.25 225)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 63 "unconnected-(U2-PC15-Pad4)")
			(pinfunction "PC15")
			(pintype "bidirectional+no_connect")
		)
		(pad "5" smd roundrect
			(at -5.675 -1.75 225)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "/OSC_IN")
			(pinfunction "PH0")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at -5.675 -1.249999 225)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "/OSC_OUT")
			(pinfunction "PH1")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at -5.675 -0.75 225)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "/NRST")
			(pinfunction "NRST")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -5.675 -0.25 225)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 82 "unconnected-(U2-PC0-Pad8)")
			(pinfunction "PC0")
			(pintype "bidirectional+no_connect")
		)
		(pad "9" smd roundrect
			(at -5.675 0.25 225)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 30 "pot_1")
			(pinfunction "PC1")
			(pintype "bidirectional")
		)
		(pad "10" smd roundrect
			(at -5.675 0.75 225)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 31 "pot_2")
			(pinfunction "PC2")
			(pintype "bidirectional")
		)
		(pad "11" smd roundrect
			(at -5.675 1.249999 225)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 62 "unconnected-(U2-PC3-Pad11)")
			(pinfunction "PC3")
			(pintype "bidirectional+no_connect")
		)
		(pad "12" smd roundrect
			(at -5.675 1.75 225)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "VSSA")
			(pintype "power_in")
		)
		(pad "13" smd roundrect
			(at -5.675 2.25 225)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "+3.3VA")
			(pinfunction "VDDA")
			(pintype "power_in")
		)
		(pad "14" smd roundrect
			(at -5.675 2.75 225)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 32 "pot_3")
			(pinfunction "PA0")
			(pintype "bidirectional")
		)
		(pad "15" smd roundrect
			(at -5.675 3.25 225)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 34 "pot_5")
			(pinfunction "PA1")
			(pintype "bidirectional")
		)
		(pad "16" smd roundrect
			(at -5.675 3.749999 225)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 35 "pot_6")
			(pinfunction "PA2")
			(pintype "bidirectional")
		)
		(pad "17" smd roundrect
			(at -3.749999 5.675 225)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 38 "pot_9")
			(pinfunction "PA3")
			(pintype "bidirectional")
		)
		(pad "18" smd roundrect
			(at -3.25 5.675 225)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "19" smd roundrect
			(at -2.75 5.675 225)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "20" smd roundrect
			(at -2.25 5.675 225)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "pot_7")
			(pinfunction "PA4")
			(pintype "bidirectional")
		)
		(pad "21" smd roundrect
			(at -1.75 5.675 225)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 39 "pot_10")
			(pinfunction "PA5")
			(pintype "bidirectional")
		)
		(pad "22" smd roundrect
			(at -1.249999 5.675 225)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 40 "pot_11")
			(pinfunction "PA6")
			(pintype "bidirectional")
		)
		(pad "23" smd roundrect
			(at -0.75 5.675 225)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 41 "pot_12")
			(pinfunction "PA7")
			(pintype "bidirectional")
		)
		(pad "24" smd roundrect
			(at -0.25 5.675 225)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 42 "pot_13")
			(pinfunction "PC4")
			(pintype "bidirectional")
		)
		(pad "25" smd roundrect
			(at 0.25 5.675 225)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 37 "pot_8")
			(pinfunction "PC5")
			(pintype "bidirectional")
		)
		(pad "26" smd roundrect
			(at 0.75 5.675 225)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 43 "pot_14")
			(pinfunction "PB0")
			(pintype "bidirectional")
		)
		(pad "27" smd roundrect
			(at 1.249999 5.675 225)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 33 "pot_4")
			(pinfunction "PB1")
			(pintype "bidirectional")
		)
		(pad "28" smd roundrect
			(at 1.75 5.675 225)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 26 "CLOCK_IN")
			(pinfunction "PB2")
			(pintype "bidirectional")
		)
		(pad "29" smd roundrect
			(at 2.25 5.675 225)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 77 "unconnected-(U2-PB10-Pad29)")
			(pinfunction "PB10")
			(pintype "bidirectional+no_connect")
		)
		(pad "30" smd roundrect
			(at 2.75 5.675 225)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 78 "unconnected-(U2-PB11-Pad30)")
			(pinfunction "PB11")
			(pintype "bidirectional+no_connect")
		)
		(pad "31" smd roundrect
			(at 3.25 5.675 225)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "Net-(U2-VCAP_1)")
			(pinfunction "VCAP_1")
			(pintype "power_out")
		)
		(pad "32" smd roundrect
			(at 3.749999 5.675 225)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "33" smd roundrect
			(at 5.675 3.749999 225)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 60 "unconnected-(U2-PB12-Pad33)")
			(pinfunction "PB12")
			(pintype "bidirectional+no_connect")
		)
		(pad "34" smd roundrect
			(at 5.675 3.25 225)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 64 "unconnected-(U2-PB13-Pad34)")
			(pinfunction "PB13")
			(pintype "bidirectional+no_connect")
		)
		(pad "35" smd roundrect
			(at 5.675 2.75 225)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 49 "unconnected-(U2-PB14-Pad35)")
			(pinfunction "PB14")
			(pintype "bidirectional+no_connect")
		)
		(pad "36" smd roundrect
			(at 5.675 2.25 225)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 55 "unconnected-(U2-PB15-Pad36)")
			(pinfunction "PB15")
			(pintype "bidirectional+no_connect")
		)
		(pad "37" smd roundrect
			(at 5.675 1.75 225)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 53 "unconnected-(U2-PC6-Pad37)")
			(pinfunction "PC6")
			(pintype "bidirectional+no_connect")
		)
		(pad "38" smd roundrect
			(at 5.675 1.249999 225)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 46 "unconnected-(U2-PC7-Pad38)")
			(pinfunction "PC7")
			(pintype "bidirectional+no_connect")
		)
		(pad "39" smd roundrect
			(at 5.675 0.75 225)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 52 "unconnected-(U2-PC8-Pad39)")
			(pinfunction "PC8")
			(pintype "bidirectional+no_connect")
		)
		(pad "40" smd roundrect
			(at 5.675 0.25 225)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 50 "unconnected-(U2-PC9-Pad40)")
			(pinfunction "PC9")
			(pintype "bidirectional+no_connect")
		)
		(pad "41" smd roundrect
			(at 5.675 -0.25 225)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 47 "unconnected-(U2-PA8-Pad41)")
			(pinfunction "PA8")
			(pintype "bidirectional+no_connect")
		)
		(pad "42" smd roundrect
			(at 5.675 -0.75 225)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 58 "unconnected-(U2-PA9-Pad42)")
			(pinfunction "PA9")
			(pintype "bidirectional+no_connect")
		)
		(pad "43" smd roundrect
			(at 5.675 -1.249999 225)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 29 "MIDI_RECEIVE")
			(pinfunction "PA10")
			(pintype "bidirectional")
		)
		(pad "44" smd roundrect
			(at 5.675 -1.75 225)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 51 "unconnected-(U2-PA11-Pad44)")
			(pinfunction "PA11")
			(pintype "bidirectional+no_connect")
		)
		(pad "45" smd roundrect
			(at 5.675 -2.25 225)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 54 "unconnected-(U2-PA12-Pad45)")
			(pinfunction "PA12")
			(pintype "bidirectional+no_connect")
		)
		(pad "46" smd roundrect
			(at 5.675 -2.75 225)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 19 "/SWDIO")
			(pinfunction "PA13")
			(pintype "bidirectional")
		)
		(pad "47" smd roundrect
			(at 5.675 -3.25 225)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "Net-(U2-VCAP_2)")
			(pinfunction "VCAP_2")
			(pintype "power_out")
		)
		(pad "48" smd roundrect
			(at 5.675 -3.749999 225)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "49" smd roundrect
			(at 3.749999 -5.675 225)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 20 "/SWCLK")
			(pinfunction "PA14")
			(pintype "bidirectional")
		)
		(pad "50" smd roundrect
			(at 3.25 -5.675 225)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 59 "I2S_WORD_SELECT")
			(pinfunction "PA15")
			(pintype "bidirectional")
		)
		(pad "51" smd roundrect
			(at 2.75 -5.675 225)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 70 "unconnected-(U2-PC10-Pad51)")
			(pinfunction "PC10")
			(pintype "bidirectional+no_connect")
		)
		(pad "52" smd roundrect
			(at 2.25 -5.675 225)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 61 "unconnected-(U2-PC11-Pad52)")
			(pinfunction "PC11")
			(pintype "bidirectional+no_connect")
		)
		(pad "53" smd roundrect
			(at 1.75 -5.675 225)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 56 "I2S_DATA")
			(pinfunction "PC12")
			(pintype "bidirectional")
		)
		(pad "54" smd roundrect
			(at 1.249999 -5.675 225)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 57 "unconnected-(U2-PD2-Pad54)")
			(pinfunction "PD2")
			(pintype "bidirectional+no_connect")
		)
		(pad "55" smd roundrect
			(at 0.75 -5.675 225)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 45 "I2S_CLOCK")
			(pinfunction "PB3")
			(pintype "bidirectional")
		)
		(pad "56" smd roundrect
			(at 0.25 -5.675 225)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 48 "unconnected-(U2-PB4-Pad56)")
			(pinfunction "PB4")
			(pintype "bidirectional+no_connect")
		)
		(pad "57" smd roundrect
			(at -0.25 -5.675 225)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "START_BTN")
			(pinfunction "PB5")
			(pintype "bidirectional")
		)
		(pad "58" smd roundrect
			(at -0.75 -5.675 225)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "MODE_SELECT_BTN")
			(pinfunction "PB6")
			(pintype "bidirectional")
		)
		(pad "59" smd roundrect
			(at -1.249999 -5.675 225)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 84 "/MODE_LED")
			(pinfunction "PB7")
			(pintype "bidirectional")
		)
		(pad "60" smd roundrect
			(at -1.75 -5.675 225)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 28 "/BOOT0")
			(pinfunction "BOOT0")
			(pintype "input")
		)
		(pad "61" smd roundrect
			(at -2.25 -5.675 225)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 83 "unconnected-(U2-PB8-Pad61)")
			(pinfunction "PB8")
			(pintype "bidirectional+no_connect")
		)
		(pad "62" smd roundrect
			(at -2.75 -5.675 225)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 44 "unconnected-(U2-PB9-Pad62)")
			(pinfunction "PB9")
			(pintype "bidirectional+no_connect")
		)
		(pad "63" smd roundrect
			(at -3.25 -5.675 225)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "passive")
		)
		(pad "64" smd roundrect
			(at -3.749999 -5.675 225)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_QFP.3dshapes/LQFP-64_10x10mm_P0.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 176.52 151.17)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "REF**"
			(at 0 -4.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "F&B.Cu" "*.Mask")
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 27.02 65.91)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "REF**"
			(at 0 -4.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "F&B.Cu" "*.Mask")
		)
	)
	(footprint "Connector_Audio:PJ-320A_PCB"
		(layer "F.Cu")
		(at 158.2 59.9 -90)
		(property "Reference" "J4"
			(at 8.4455 -3.269 -90)
			(layer "F.SilkS")
		)
		(property "Value" "LINE_OUT_R"
			(at 8.4455 -4.539 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Audio:PJ-320A_PCB"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Jack"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "-"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "DAC")
		(sheetfile "DAC.kicad_sch")
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at 3.7 2.2 270)
			(size 1.1 1.1)
			(drill 1.1)
			(layers "F&B.Cu")
		)
		(pad "" thru_hole oval
			(at 5.15 0 270)
			(size 1.8 1.5)
			(drill oval 1.4 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "" np_thru_hole circle
			(at 10.7 2.2 270)
			(size 1.1 1.1)
			(drill 1.1)
			(layers "F&B.Cu")
		)
		(pad "R" thru_hole oval
			(at 8.25 0 270)
			(size 1.8 1.5)
			(drill oval 1.4 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "unconnected-(J4-PadR)")
			(pintype "passive+no_connect")
		)
		(pad "S" thru_hole roundrect
			(at 13.45 4.5 270)
			(size 1.7 1.6)
			(drill oval 1.4 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.1470588235)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "T" thru_hole oval
			(at 12.35 0 270)
			(size 1.8 1.5)
			(drill oval 1.4 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "Net-(C26-Pad1)")
			(pintype "passive")
		)
		(model "/Users/mortenslingsby/Documents/DIY/5. KiCad lib/PJ-320a/PJ-320A.step"
			(offset
				(xyz 2 -2.4 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 163.976 90.3 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R12"
			(at 0 -1.43 180)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.43 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C21190"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Interface")
		(sheetfile "Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 80 "Net-(SW3-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "MODE_SELECT_BTN")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 108.64 90.775 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "FB1"
			(at -0.021 -2.468 0)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.68 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ferrite bead"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C1017"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Inductor_* L_* *Ferrite*")
		(sheetname "Root")
		(sheetfile "Drumbadum.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "+3.3VA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 101.55 127.5)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 2.25 0.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C307331"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Drumbadum.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "/NRST")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 161.351 105.782 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C27"
			(at -2.023 -0.808 180)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C307331"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Interface")
		(sheetfile "Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "START_BTN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 166 82.5 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R3"
			(at 0.75 1.5 180)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.43 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C21190"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Drumbadum.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "Net-(D2-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 84 "/MODE_LED")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 91.0572 109.2708 -135)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C9"
			(at 0.501622 2.18991 0)
			(layer "F.SilkS")
		)
		(property "Value" "2.2u"
			(at 0 1.679999 -135)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 -135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C377773"
			(at 0 0 -135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Drumbadum.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -135)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.949999 0 225)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "Net-(U2-VCAP_1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.949999 0 225)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 98.034789 121.1326 -45)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C10"
			(at 139.148008 -6.282644 135)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 135)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C307331"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Drumbadum.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 135)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 315)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 315)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 163.891 105.274 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R6"
			(at -0.046 -1.533 180)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.43 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C21190"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Interface")
		(sheetfile "Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 79 "Net-(SW2-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "START_BTN")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 116.35 112.35 135)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 0.551543 -1.428356 0)
			(layer "F.SilkS")
		)
		(property "Value" "20p"
			(at 0 1.16 -45)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LSC Part No" "C1554"
			(at 0 0 135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Drumbadum.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -45)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 135)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "/OSC_IN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 135)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 75.91 109.25 180)
		(property "Reference" "~"
			(at 0 0 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(gr_rect
		(start 23.0292 61.8488)
		(end 180.2792 155.0816)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_text "- Jon Bon Jovi, 1985 (year of the ox)"
		(at 151.82 137.11 0)
		(layer "B.SilkS")
	)
	(gr_text "FOOLS DRUMS V1.0"
		(at 147.46 67.07 0)
		(layer "B.SilkS")
	)
	(gr_text "{dblquote}Don't overthink;\n  underthink{dblquote}"
		(at 163.67 133.34 0)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 105.6 145.7 270)
		(layer "F.SilkS")
	)
	(gr_text "SWDIO"
		(at 98 145.5 270)
		(layer "F.SilkS")
	)
	(gr_text "+3.3V\n"
		(at 95.4 145 -90)
		(layer "F.SilkS")
	)
	(gr_text "NRST"
		(at 100.5 145.5 270)
		(layer "F.SilkS")
	)
	(gr_text "FOOLS\nDRUMS"
		(at 69.74 104.7 0)
		(layer "F.SilkS")
	)
	(gr_text "SWCLK"
		(at 103.1 145.6 270)
		(layer "F.SilkS")
	)
	(zone
		(net 3)
		(net_name "+3.3V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads yes
			(clearance 0.3)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.3)
		)
		(polygon
			(pts
				(xy 93.875 79.95) (xy 93.875 77.35) (xy 95.95 77.35) (xy 95.95 81.525) (xy 101.45 81.85) (xy 101.85 82.2)
				(xy 103.225 82.2) (xy 103.225 83.175) (xy 97.275 83.175) (xy 97.3 86.15) (xy 92.575 86.15) (xy 92.6 83.575)
			)
		)
	)
	(zone
		(net 86)
		(net_name "/VBUS")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads yes
			(clearance 0.3)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.3)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 91.625 79.875) (xy 91.625 77.025) (xy 93.325 75.125) (xy 94.65 75.125) (xy 94.65 76.95) (xy 93.925 76.95)
				(xy 93.475 77.375) (xy 93.475 79.875)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads yes
			(clearance 0.3)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.3)
		)
		(polygon
			(pts
				(xy 94.945 75.9808) (xy 94.95 74.775) (xy 97.45 74.8) (xy 103.27 80.2) (xy 103.25 81.99) (xy 101.96 81.99)
				(xy 101.675 81.6) (xy 101.475 81.325) (xy 99.3 81.325) (xy 98 80.825) (xy 96.25 80.8) (xy 96.279162 77.3)
				(xy 95.86 76.88) (xy 94.96 76.9)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+3.3V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads yes
			(clearance 0.3)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.3)
		)
		(polygon
			(pts
				(xy 97.275 83.85) (xy 98.1 83.175) (xy 97.075 83.1) (xy 97.275 83.825)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+3.3V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.3)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.3)
		)
		(polygon
			(pts
				(xy 95.9 80.9) (xy 96.65 81.65) (xy 95.75 81.65) (xy 95.875 80.9)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 18.923 60.9854) (xy 183.1594 61.5442) (xy 183.1594 159.8422) (xy 18.3388 159.2326) (xy 18.796 61.9506)
			)
		)
	)
)