(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(grid_origin 133.9658 51.5992)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions yes)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue no)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk yes)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "../Gerber/front_panel/")
		)
	)
	(net 0 "")
	(footprint "LOGO"
		(layer "F.Cu")
		(at 72.3708 103.6692)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 95.975297 119.885689 25)
		(property "Reference" "G***"
			(at 0 0 25)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 25)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 25)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 25)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 25)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 109.9158 121.1192 -25)
		(property "Reference" "G***"
			(at 0 0 155)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 -0.000001 155)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -25)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -25)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -25)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 143.8658 109.3792)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 125.8378 51.4722)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 210.325249 89.9492)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 134.1058 73.0792)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(gr_circle
		(center 99.187 103.692)
		(end 102.937 103.692)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 120.452727 124.567649)
		(end 124.202727 124.567649)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 186.388654 61.94762)
		(end 190.138654 61.94762)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 210.646356 84.070937)
		(end 213.646356 84.070937)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 161.525387 124.578807)
		(end 165.275387 124.578807)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_rect
		(start 56 43.95)
		(end 227.25 141.952)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 59.4658 138.1992)
		(end 60.9658 138.1992)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 143.0498 51.5992)
		(end 145.0498 51.5992)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 133.9658 51.5992)
		(end 136.4658 51.5992)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 210.646356 100.987237)
		(end 214.396356 100.987237)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 210.646356 60.8692)
		(end 212.646356 60.8692)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 210.646356 69.9592)
		(end 213.646356 69.9592)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 223.7158 138.1992)
		(end 225.2158 138.1992)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 59.5 47.145)
		(end 61 47.145)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 184.257221 124.581898)
		(end 188.007221 124.581898)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 176.477435 82.795286)
		(end 180.227435 82.795286)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 89.761466 82.793193)
		(end 93.511466 82.793193)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 159.474377 61.913478)
		(end 163.224377 61.913478)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 223.75 47.145)
		(end 225.25 47.145)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 210.646356 119.989434)
		(end 214.396356 119.989434)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 113.3006 61.9184)
		(end 117.0506 61.9184)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 72.39 103.692)
		(end 72.39 99.942)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 85.756897 124.584973)
		(end 89.506897 124.584973)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 70.805418 61.905171)
		(end 74.555418 61.905171)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_text "SOUND"
		(at 137.1158 118.6492 0)
		(layer "F.SilkS")
	)
	(gr_text "FOOLS"
		(at 107.8458 90.6192 0)
		(layer "F.SilkS")
	)
	(gr_text "OUT"
		(at 199.8958 48.2942 0)
		(layer "F.SilkS")
	)
	(gr_text "MIDI IN"
		(at 76.1058 48.8542 0)
		(layer "F.SilkS")
	)
	(gr_text "VOL\n"
		(at 207.224737 130.663803 0)
		(layer "F.SilkS")
	)
	(gr_text "CLK IN"
		(at 92.0258 48.9042 0)
		(layer "F.SilkS")
	)
	(gr_text "R"
		(at 208.3958 48.8042 0)
		(layer "F.SilkS")
	)
	(gr_text "MODE"
		(at 205.097693 77.732463 0)
		(layer "F.SilkS")
	)
	(gr_text "BPM"
		(at 206.145249 111.9692 0)
		(layer "F.SilkS")
	)
	(gr_text "SEQUENCE"
		(at 125.25 67.052 0)
		(layer "F.SilkS")
	)
	(gr_text "L"
		(at 194.7758 48.8742 0)
		(layer "F.SilkS")
	)
	(gr_text "DRUMMMS"
		(at 128.8858 104.4312 0)
		(layer "F.SilkS")
	)
	(gr_text "10111010"
		(at 172.5158 71.5492 285)
		(layer "F.Mask")
	)
	(gr_text "SWITCH"
		(at 207.817693 70.702463 0)
		(layer "F.Fab")
	)
	(gr_text "ON/\nOFF"
		(at 132.3858 53.0692 0)
		(layer "F.Fab")
	)
	(gr_text "SWITCH"
		(at 207.715249 84.7892 0)
		(layer "F.Fab")
	)
	(gr_text "LED"
		(at 141.8658 52.1992 0)
		(layer "F.Fab")
	)
	(gr_text "LED"
		(at 209.1498 61.7592 0)
		(layer "F.Fab")
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 1)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 49.45 39.252) (xy 234.95 38.352) (xy 238.75 155.352) (xy 41.25 149.152)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 231.9658 145.6992) (xy 232.6658 38.4992) (xy 48.2658 40.3992) (xy 50.1658 146.0992) (xy 233.1658 144.6992)
			)
		)
	)
)